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Wine / Beverage Preservation Technology


 (
INSTRUCTION MANUAL
)

BV60S
BV60BL
BV600TBL
WCDZ60S
WCDZ60BL
WCBV60BL
WCDZ600TS
WCDZ600TBL
WCDZ601T
WCDZ60INT/1
WCSZ45BL
WCSZ60BL
WCSZ605BL
BV60INT/1
BV60DRAWINT
Thanks for buying one of our Wine or Beverage cabinets. Before use, please  read  and follow all safety rules and operating instructions.
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 (
WARNING
)

The information in this document is subject to modification without prior notice. Some models are available in dedicated countries only.

All warranties are void if the appliance is being used for any purpose other
than that for which it was specifically designed. Warranty applies to the wine cabinet only and not to the content of the wine cabinet.

This appliance is not intended for use by persons (including children) with
reduced physical, sensory or mental capabilities, or lack of experience and
knowledge, unless they have been given supervision or instruction concerning use of the appliance by a person being responsible for their safety. Children
shall not play with the appliance. Cleaning and user maintenance shall not be made by children without supervision.

Children should be supervised to ensure that they do not play with the appliance.

Please don't put acidic items, flammable and explosive goods into wine cabinet.

This appliance is intended to be used exclusively for the storage of wine and beverage.

This appliance is not suitable for freezing foodstuffs.

This appliance is intended to be used in household and similar applications such as
- Staff kitchen areas in shops, offices and other working environments;
- Farm houses and by clients in hotels, motels  and other residential type
environments;
- Bed and breakfast type environments;
- Catering and similar non-retail applications.

DANGER: Risk of child entrapment. Before you throw away your old 
wine chiller:

- Take off the doors;
- Leave the shelves in place so that children may not easily climb inside;
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- When disposing of the appliance, do so only at an authorized waste disposal centre.

 (
R600a WARNINGS
)
For your safety observe the following recommendations.
.  This appliance contains a small quantity of R600a refrigerant which is   environmentally friendly, but flammable.  It does not damage the ozone layer, nor does it increase the greenhouse effect.
.  During transportation and installation, ensure that the tubing of the refrigerant circuit is not damaged.
.  Avoid using sharp objects near by the appliances.
.  Leaking refrigerant can ignite and may damage the eyes.
.  In the event any damage does occur, avoid exposure to open fires and any device which creates a spark.  Disconnect the appliance from the mains
power.
.  Thoroughly ventilate the room in which the appliance is located for several minutes.
.  Notify Customer Service for necessary action and advice.
.  The room you installing the appliance in must be at least 1 cubic metre per 8 grams of refrigerant.  The refrigerant quantity contained in this
appliance is listed on the Rating Plate of the appliance.

It is hazardous for anyone other than an Authorized Service Person to carry out servicing or repairs to this appliance.

- WARNING: Keep ventilation openings in the appliance enclosure or in the built-in  structure clear of obstruction.
- WARNING: Do not use mechanical devices or other means to accelerate  the defrosting process, other than those recommended by the manufacturer.
- WARNING: Do not damage the refrigerant circuit.
- WARNING: Do not use electrical appliances inside the food storage
compartments of the appliance, unless they are of the type recommended by the manufacturer.
- WARNING: If you are not using the appliance, please unplug the power plug from the socket or switch off the power supply.
- WARNING: This appliance is not intended for use by persons (including children) with reduced physical, sensory or mental capabilities, or lack of  experience and knowledge, unless they have been given supervision or
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instruction concerning use of the appliance by a person responsible for their safety.
- WARNING:Children should be supervised to ensure that they do not play with the appliance;
- WARNING: Do not use extension cords or ungrounded (two prong) adapters.
- WARNING: If the supply cord is damaged, it must be replaced by the manufacturer,Its service agent or similar qualified person in order to
avoid hazard.

Allow 24 hours before switching on the wine cabinet. During this time we recommend that you leave the door open to clear any residual odors.

BEFORE LOADING & PLUGGING IN THE WINE CABINET

Important: All models without front venting (air opening) are strictly for free standing only. (See technical chart)

Recommendations:
The location you have selected for your wine cabinet should:
- Be unencumbered and well ventilated;
- Be well away from any heat source and direct sunlight;
- Not be too damp (laundry, pantry, bathroom etc.);
- Have a flat floor;
- Have a standard and reliable electricity supply (standard socket to country standards, linked to the ground), it is NOT recommended to use a multi-socket or extension lead;
- Have a surge protector fitted to the electrical outlet;
- Away from the microwave oven. Certain microwave ovens do not have wave interference shield. When placed within 1 meter vicinity of the wine cabinet, they may affect the operation of the wine cabinet.


Wine cabinet should be placed where the ambient temperature is constant (not to hot or cold). If the temperature is too hot or cold, it will affect the performance of the cabinet.

Grounding instructions:
The wine cabinet must be grounded in case of power leakage. Grounding reduces the risk of electrical shock. The wine cabinet is equipped with a power cord having an earth wire and an earthed plug. The wine cabinet plug must be plugged into a grounded electrical outlet.

Note:  In locations where there is frequent lightning, it is advisable to use surge protectors.
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Improper use of the earthed plug can result in the risk of electric shock. Consult a qualified electrician or service person if the grounding instructions are not completely understood.
If the supply cord is damaged, it must be replaced by a qualified person in order to avoid electrical hazard.

INSTALLING YOUR WINE CABINET

Unpack and remove all of the protection and adhesive strips from the packaging around and inside the wine cabinet.
The wine cabinet must be positioned such that the plug is accessible. Release the power cord. Move your wine cabinet to its final location. The wine cabinet should be installed in a suitable place where the compressor will not be subject to physical contact.

Leveling your wine cabinet: Wine cabinet must be leveled BEFORE loading your wines.

Your wine cabinet is equipped with 4 adjustable feet to facilitate easy leveling. We
recommends that you tighten the back feet to the maximum and adjust the front feet to level the wine cabinet.


INSTALLATION INSTRUCTIONS FOR BUILT IN WINE CABINETS: (UNDERBENCH OR IN COLUMN) FRONT VENTING WINE CABINETS ONLY.



1. “Built in” wine cabinets are front venting but are not designed to be fully integrated behind a joinery door.

2. Please follow the installation diagram when installing built-in wine cabinets. No less than the minimum installation dimension, or it will affect the venting of cabinet.

3. Built-in wine cabinets draw air from right of ventilation frame and expel through left of ventilation frame under the front door.

4. “Built in” wine cabinets have a power switch located on the control panel so 
power point location is not critical.

5. The wine cabinet requires a standard 240 volt/10 amp power point.

6. The power cord is 2.0m in length and is fixed on the right side at the back when looking from front of cabinet.
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7. As with most appliances of today, the wine cabinet has sensitive electronic components which  are  susceptible  to  damage  through  lightning  and  electricity  supply  faults.  It  is therefore advised to use a power surge protector to avoid problems of this nature.

8. Air  vent  on  door  must  be  provided  for  built-in  wine  cabinets  when  a  wood  door installed.

In Hot climate zone, an air vent or grid, with a minimum ventilation size of 200mm x 40mm MUST be cut out at the rear top of the back partitioning or at the top of either side of the partitioning, allowing cool fresh air full access to flow into the 30mm gap located at the rear of the cabinet.

This air vent or grid must not be opened on the same side as other appliances such as ovens or an area that is sealed and without access to fresh cool air. Failing to comply with the above specifications will void the WARRANTY.


INSTALLATION  DRAWINGS FOR BUILT IN WINE CABINETS: (UNDERBENCH OR IN COLUMN) FRONT VENTING WINE CABINETS ONLY.
Note: The appliance must be positioned so that the plug is accessible after installed.

 (
DIMENSIONAL  DRAWINGS:
)

WCSZ45BL
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Installation Instruction:

[image: ]
1. Put the wine cooler into the cabinet, then adjust the wine cooler to make it steady. Open the door, take out the fixed plate , 2pcs Inner Hexagon Screws ,and Inner Hexagon
Screwdriver from accessory bag , then use the inner hexagon screwdriver to tighten the fixed plate on the lower left side of wine cooler.
2. Take out 3pcs Phillips screws from accessory bag , use Phillips  screwdriver to tighten  the fixed plate on the lower left side of wine cooler(1pcs screw) , then tighten the other 2pcs Phillips screws on the upper door hinge and lower door hinge.
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BV60BL, BV60S, WCDZ60BL, WCDZ60S, WCSZ60BL
leave min. 20mm gap at the rear of the appliance

[image: ]


 (
WCDZ60INT/1, BV60INT/1
DO NOT COVER VENT!
)





BV60DRAWINT
[image: IMG_256]
After the door panel is fully adjusted, take out 12 self-tapping crews of ST4*35 from the accessory bag, remove the door seal, drill the screws through the screw holes on door frame, and then tighten the door panel.

WCSZ605BL
leave min. 20mm gap at the rear of the appliance
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WCDZ600TS, WCDZ600TBL, WCDZ601T, BV600TBL
leave min. 20mm gap at the rear of the appliance

[image: ]

OPEN  ANGLE  SIZE  DRAWINGS:


WCSZ45BL
[image: ]
BV60BL, BV60S, WCDZ60BL, WCDZ60S, WCSZ60BL
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WCBV60BL


[image: ]
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WCDZ60INT/1, BV60INT/1

[image: ]

WCSZ605BL
[image: ]
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WCDZ600TS, WCDZ600TBL, WCDZ601T, BV600TBL

[image: ]

[image: ]BV60DRAWINT
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 (
RADIATOR SYSTEM DESC
RIPTION
)

BV60BL, BV60S, WCDZ60BL, WCDZ60S, WCBV60BL, WCDZ600TS, WCDZ600TBL, WCDZ601T, BV600TBL, WCDZ60INT/1, WCSZ60BL, BV60INT/1,  WCSZ605BL models use side anti-dew tube and Independent cooling system:
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BV60DRAWINT models use side anti-dew tube and Independent cooling system:

[image: ]
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WCSZ45BL  model use a rear cooling system.
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TURNING ON YOUR WINE CABINET

Plug in and switch on the cabinet by pressing on the power button for a few seconds.
When you use the wine cabinet for the first time (or restart the wine cabinet after having it shut off for a long time), there will be a few degrees variance between the temperature you have selected and the one indicated on the LED readout.  This is normal and it is due to the  length  of the  activation  time.  Once  the  wine  cabinet  is  running  for  a  few  hours everything will stabilize.

Important: If the unit is unplugged, power is lost, or turned off, wait 3 to 5 minutes before restarting the unit. The wine cabinet will not start if you attempt to restart before this time delay.

Operating Noises
To reach the desired temperature settings, our wine cabinets, like all wine cabinets
operating with compressors and fans, may produce the following types of noises. These noises are normal and may occur as follows:
-  Gurgling sound - caused by the refrigerant flowing through the appliance’s coils.
-  Cracking/popping sounds - resulting from the contraction and expansion of the refrigerant gas to produce cold.
-  Fan operating sound - to circulate the air within the wine cabinet.
An individual’s perception of noise is directly linked to the environment in which the wine cabinet is located, as well the specific type of models. Our wine cabinets are in line with   international standards for such appliance. We will always do its utmost to satisfy its
customers but will not retake possession of the goods due to complaints based on normal operating noise occurrences.

 (
LOADING YOUR WINE CABINET
)

You may load your wine bottles in single or double rows while taking note of the following: if you do not have enough bottles to fill your wine cabinet, it is better to distribute the load throughout the wine cabinet so as to avoid“all on top”or“all below”type loads.
- Do remove or relocate adjustable wooden shelves to accommodate larger type of bottles or increase the capacity of the cabinet by stacking the bottles up when necessary. (See removing shelves)
- Keep small gap between the walls and the bottles to allow air circulation. Like an underground cabinet air circulation is important to prevent mould and for a better homogeneous temperature within the cabinet.
[image: ]

-  Do not over load your wine cabinet to facilitate air circulation.
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- Do not stack more than 1.5 rows of standard 0.75L bottles per shelves to facilitate air circulation
-  Avoid obstructing the internal fans (located inside on the back panel of the wine cabinet).
- Do not slide the shelves outwards beyond the fixed position to prevent the bottles from falling.
- Do not pull out more than one loaded shelf at a time as this may cause the wine cabinet to tilt forward.
- Do not cover the wooden shelves with alloy foil or other materials, as it will obstruct air circulation.
- Do not move your wine cabinet while it is loaded with wines. This might distort the body of the wine cabinet and cause back injury.

 (
TYPES OF REGULATION
)

Please note that depending on the loading and settings chosen it takes about 24 hours for the wine cabinet to see the temperature stabilizing.
During this time LED seems to move erratically in particular, it is normal and this process occurs whenever the setting is modified and/or whenever a large amount of bottles are added to the cabinet.

Designed to store and mature all wines: red, white and sparkling. These wine cabinets
reproduce the ideal conditions for wine storage, at a constant recommended temperature of 12ºC.  They can also be set to provide ideal serving temperature for full enjoyment of the    wine’s qualities. Unless stated by the wine maker on the bottle, we recommends 7ºC for
your champagne, 12ºC for whites and 18ºC for reds. (Refer to “Wine Service Temperature” recommendation chart)
TEMPERATURE SETTINGS

Important: The LED displays by default shows the actual internal air temperature.

In the event of loss of power the unit will return to your preset temperatures when turned back on.

The electrical board of all models comes with memory function.
It is important to understand that there is a difference between the air temperature inside the  wine  cabinet  and  the  actual  temperature  of  the  wine:  You  will  need  to  wait approximately 12 hours before noticing the effects of temperature adjustment due to the critical mass within a full wine cabinet.

Once the temperature is set, it is strongly advised not to toy with it or adjust frequently. The thermostat will maintain the temperature inside the wine cabinet within a +/- 2.5ºC range. But the thermal inertia of the wine and the glass is such that within this temperature range, the actual temperature of the wine will only fluctuate 0.5ºC to 1ºC.
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WCBV60BL,WCSZ45BL SINGLE  
TEMPERATURE
  DISPLAY BO
ARD
)
 (
OPERATING INSTRUCTION:
)
[image: ]

[image: ] ① Display Window:
Display the measured temperature inside the wine cabinet;

[image: ] ② Temperature Setting / Cycle Icon：
Each time, the temperature inside will drop 1 ℃, until reduced to a minimum, and then a return to the highest temperature.

Press and hold for 3 seconds, the window to achieve Celsius / Fahrenheit display conversion
[image: ] ③ Lighting / Power Icon：
In standby mode: press and hold for 3 seconds, power is turned on, the machine starts;   When power on, press the icon and hold for 3 seconds, power is off, the machine is off. Each short touch on this icon: LED lighting on / off


BV60BL, BV60S, BV600TBL, WCSZ60BL, BV60INT/1, BV60DRAWINT,
WCSZ605BL SINGLE TEMPERTURE DISPLAY BOARD OPERATING
OPERATION:

[image: ]


[image: ] ①Energy Saving Mode
Press the icon and hold for 3 seconds into the energy-saving mode, press ⑥⑦ out of energy-saving mode
[image: ] ②ON/OFF Power Icon:
In the standby mode: press and hold for 3 seconds, the power is turned on, the whole machine starts
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In the power-on state: press and hold for 3 seconds, window 4 shows the countdown 3 2 1, then power is turned off, the machine is turned off (show 3 2 1 process, the hand cannot
leave the button)

[image: ] ③Lighting Icon:
Each short touch on this icon: LED lighting on / off

[image: ] ④ Display Window:
Displays the setting temperature

[image: ] ⑤Display Window:
Displays the actual temperature

[image: ] ⑥Temperature Setting Up Icon :
Press one time, In window ④ the setting temperature will increase by 1 degree Celsius (Max. Setting Temperature: 10℃).

[image: ] ⑦Temperature Setting Down Icon :
Press one time, In window ④ the setting temperature will decrease by 1 degree Celsius (Min. Setting Temperature: 2℃).

[image: ] ⑧C/F Temperature Display Conversion Function Icon:
Press and hold for 3 seconds, the window to achieve Celsius / Fahrenheit display conversion

WCDZ60S WCDZ60BL WCDZ600TS, WCDZ601T, WCDZ60INT/1  DUAL TEMPERTURE DISPLAY BOARD OPERATING INSTRUCTION:

[image: ]

[image: ] ①ON/OFF Power Icon:
In the standby mode: press and hold for 3 seconds, the power is turned on, the whole machine starts

In the power-on state: press and hold for 3 seconds, window 4 shows the countdown 3 2 1, then power is turned off, the machine is turned off (show 3 2 1 process, the hand cannot
leave the button)

[image: ] ②Temperature Setting Up Icon (Upper Zone) :
Press one time, In window ④ the setting temperature will increase by 1 degree Celsius
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(Max. Setting Temperature: 20℃).

[image: ] ③Temperature Setting Down Icon (Upper Zone) :
Press one time, In window ④ the setting temperature will decrease by 1 degree Celsius (Min. Setting Temperature: 10℃).

[image: ] ④Window :
Display upper zone temperature.

[image: ] ⑤Window:
Display lower zone temperature

[image: ] ⑥Temperature Setting Up Icon (Lower Zone) :
Press one time, In window  ⑤ the setting temperature will increase by 1 degree Celsius (Max. Setting Temperature: 12℃.).

[image: ] ⑦Temperature Setting Down Icon (Lower Zone) :
Press one time, In window ⑤ the setting temperature will decrease by 1 degree Celsius (Min. Setting Temperature: 5℃.).

[image: ] ⑧Lighting Icon:
Each short touch on this icon: LED lighting on / off.

[image: ] ⑧C/F Display Conversion Function Icon:
Press and hold for 3 seconds,  the window to achieve Celsius / Fahrenheit display conversion

 (
WINE SERVING TEMPERATURE
 CHART
)

All wines mature at the same temperature, which is a constant temperature set between 12ºC to  14ºC.  The  below  chart is an indicative temperature chart to indicate the best temperature for drinking purposes.

Champagne NV, Sparkling, Spumante                                                                                6ºC
Dry White Semillon, Sauvignon Blanc                                                                                8ºC
Champagne Vintage,                                                                                                          10ºC
Dry White Chardonnay                                                                                                       10ºC
Dry White Gewürztraminer, Riesling, Pinot grigio                                                           10ºC
Sweet White Sauternes, Barsac, Montbazillac, Ice Wine, Late Harvest                           10ºC
Beaujolais                                                                                                                            13ºC
Sweet White Vintage: Sauternes …                                                                                     14ºC
White Vintage Chardonnay                                                                                                14ºC
Red Pinot Noir,                                                                                                                   16ºC
Red Grenache, Syrah                                                                                                           16ºC
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Red Vintage Pinot Noir                                                                                                      18ºC
Cabernet & Merlot                                                                                                             20ºC
Chilean, Italian, Spanish, Californian, Argentinean …
Vintage Bordeaux …                                                  Room temperature not exceeding 20ºC


IMPORTANT INFORMATION ABOUT TEMPERATURE

Your wine cabinet has been designed to guarantee optimum conditions for storing and/or serving your wines.

Fine wines require long and gentle developments and need specific conditions in which to reach their full potential.

All wines mature at the same temperature, which is a constant temperature set between 12ºC to 14ºC. Only the temperature of “degustation” (wine appreciation) varies according to the type of wines (see “Wine Serving Temperature Chart” above).  This being said and as it is for natural cabinets used by wine producers for long period of storage, it is not the exact temperature that is important, but its consistency. In other words, as long as the temperature of your wine cabinet is constant (between 12ºC to 14ºC) your wines will be stored in perfect conditions.

Not all wines will improve over the years. Some should be consumed at an early stage (2 to 3 years) while others have tremendous ageing capability (50 and over). All wines have a peak in maturity. Do check with your wine merchant to get the relevant information.

DEFROSTING/ CONDENSATION/ HYGROMETRY/ VENTILATION

Defrost water from the wine cabinet storage compartment drains automatically and part of it goes into a drainage container, which is located at the back of the wine cabinet next to the  compressor.  The  heat  is  transferred  from  the  compressor  and  evaporates  any condensation that has collected in the pan. Part of the remaining water is collected within the wine cabinet for humidity purposes.
This system enables the creation of the correct humidity level inside your wine cabinet required by the natural cork to maintain a long lasting seal.
Notes: The water collected by condensation, is therefore recycled. Under extremely dry environmental conditions, you may have  to  add some water  into  the  water container provided with your wine cabinet.

All units are equipped with a double glazed glass door that has a third internal acrylic layer to minimize condensation on the glass door.

The  wine  cabinet  is  not  totally  sealed;  fresh  air  admission  is  permitted  through  the drainpipe.   Air is circulated through the cabinet by means of a  fan/fans and the hollow shelves.
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Notes: During the refrigerating cycle, heat is given offand disperses through the external surfaces ofthe wine cabinet. Avoid touching the surfaces during those cycles.

 (
BV
60
BL
, 
BV
60S, 
WCDZ
60
BL
,
WCDZ
60S, 
WCBV
60
BL
, 
WCSZ
605
BL
 
SMALL HANDLE INSTALLATION I
NSTRUCTION
)

1. Take the small handle and 2x screws from the accessory bag inside the cabinet.
2. Remove 2 x screw covers on top door frame and mount the small handle on top door frame, tighten it with screws by a Phillips screwdriver.

[image: ]

 (
ADJUSTABLE WOODEN SHELVES
)

Shelf installation and taking instruction:
Common wooden shelf:
Shelf taking: According to below instruction drawing to press one side of shelf limit pin①, extract and remove the shelf from the other side of support bracket ② , then take off the shelf following the arrow mark ③.
Shelf installation will be opposite with shelf taking.

[image: ]
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1、”A” is shelf limit pin          2 、”B” is shelf
Sliding wooden shelf installation and taking instruction:
Shelf taking: According to below instruction  drawing to pull out the  shelf to  support bracket ①, press two sides of sliding roller buckles and pull out the shelf following the arrow mark ②.

Shelf installation: According to below instruction drawing to push in the shelf alignment with two sides of sliding roller following the arrow mark ③.

[image: ]


 (
REV
ERSIBILITY OF TH
E DOO
R
)

REMARK:
If your wine cabinet has a lock at the bottom of the door, the door is irreversible and only the door that op ens to the left or right can be reversed.

Warning: To avoid accidents during the process of changing the door, we recommend that you get assistance. The glass door is heavy and may cause injury if dropped.
- Depending on to the model and the type of handle your wine cabinet is equipped with, you may have to rotate the door through 180 degrees.
- Depending on the type of handle your wine cabinet is equipped with, the door may not be reversible or may require that a left or right opening door be ordered to change the opening side.

 (
REV
ERSIBILITY OF TH
E DOO
R
)

BV60BL, BV60S, WCDZ60BL, WCDZ60S, WCBV60BL, WCDZ600TS, 
WCDZ600TBL, WCDZ601T, BV600TBL, WCSZ60BL, WCSZ605BL will use same method to install the door

1. To put the cabinet on open operation place, the door opened to the maximum angle
2. Use small knife(2) to take off the decorative nail (1) on opposite side (Drawing 1);
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3. Use the inner six angle screwdriver (Tool 5) to disassemble the screws(4) of drop-proof device (3), then remove the drop-proof device .(Drawing 1)
4. Hold the door, use six angle screwdriver (Tool 5) to screw out the door shaft core(6) from the two ends of the top of the door. Take out the door and set aside. (Drawing 2)
5. Discharge the upper and lower door hinge(7)(8) by M5 inner six angle screwdriver (Tool 5) , then to assemble the door hinge on the opposite side. (Drawing 3 and 4 )
6. Rotate the door 180 degrees, then Install the door on the right side of the cabinet. (Drawing 5)
7. Finally, install the decorative nail and drop-proof device at the opposite side. (Drawing 6)
[image: ]
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1.Decorative nail                          2. Knife                                        3. Drop-proof device

4. M5 six angle                              5. M5 six angle screwdriver        6. Door spindle core

7. Upper door hinge                      8. Lower door hinge


WCDZ60INT/1, BV60INT/1  will use follow method to install the door

1.Put the cabinet in an open operating area, have the door opened to the maximum angle.

2. Use the knife ② to remove the decorative nails ① from the  left side of the cabinet. (Figure 1)


3. Use the Phillips screwdriver④ to remove the M5 Phillips countersunk screw③ that fix the upper and lower door hinges. (Figure 2)

[image: ]
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4. Rotate the door by 180 degrees, and install it to the other side of the cabinet. (Figure 3 and 4)

[image: ]
5. At last, install all decorative nails to the other side of the door①, door installation is all set! (Figure 5)



BV60DRAWINT Drawer Disassembly Method

1. Pull  the  drawer  (1)  outward  to  the  max.  position,  and  remove  the  screws  (3)  on  the drawer (1) and the sliding rail (2) on both sides with a Phillips screwdriver.
(See Figure 1)
2. Lift the drawer (1) up, so that both sides of the drawer out of the front buckle (4), you can take out the drawer. (See Figure 2)
3. Install drawers in the opposite way. Pay attention to the buckle (4) in correct place during installation.

[image: IMG_256]

 (
WCSZ45BL will use follow method to install the
 door
)

Warning: To avoid accidents during the process of changing the door, we recommend that you get assistance. The glass door is heavy and may cause injury if dropped. Please turn
off the power before reversing the door.

1. Use knife to pry the six trunk-nails from left side of cabinet. Please be careful, don’t hurt the hands and don’t damage the surface of cabinet (Picture 1)

2. Open the door, use Phillips screwdriver to loosen the screws of upper and lower door hinge, and then remove the door (Picture 2)

3. Then use hexagon wrench to loosen the screws of upper and lower door hinge, remove  the door hinge, and then install upper door hinge at lower opposite side, install lower door hinge at upper opposite side (Picture 3)
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4. The upper and lower ends of the removed door are directly aligned with the door hinges on the left side of the cabinet, adjust the door, and tighten the upper and lower screws with a Phillips screwdriver to complete the door replacement. Then install six trunk-nails to
right side (Picture 4 & Picture 5)

5. After closing the door, check whether the probe on the door frame is aligned with the metal plate on the cabinet. If it is not aligned, loosen the screws on the upper and lower  door hinges and adjust the door until it is aligned (Picture 6)

6. Plug in the power, find the press sign, and slowly press twice, if the door can be opened, the reversible door is successful.


1. Knife   2.   Trunk nails   3. Phillips Screwdriver   4. Screw   5. Upper door hinge
6.Allen driver   7. Lower door hinge   8. Probe   9. Metal plate

[image: ]
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[bookmark: _GoBack]BV60DRAWINT Tilt-prevention Kit Mounting Instruction for Free-standing 
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Mounting on Device
Mounting on wall Connecting two plates
30mm


Device
50~70mm

Figure 1. Side view




Device                                                                                    Wall
Align two plates and ﬁx.

Figure 2. Top view

1. Accessories:
Metal fixation plates          2pcs
M5*16 ﬂat head screws    3pcs
ST4*30 ﬂat head self-tapping screws   2pcs
M6*60 Anchors           1pcs
2. Instruction:
a. Adjust device feet to level the device;
b. Place the metal fixation plates according to Figure 1, and ﬁx one to the device with
M5*16 flat head screws (screw holes drilled) , the other one to the wall with M6*60 anchor; ST4*30 ﬂat head self-tapping screws can be used on wooden wall. (Please
consult a professional for the application of screws if necessary. )
c. Move the device in order to overlap the two metal fixation plates partly, keep a distance between backboard and wall at around range of 50-70mm. Fix the two metal plates with two M5*16 screws.
3. The adjustable distance can be 50mm, 60mm, 70mm--Figure 3.

Figure 3

AUTO-DOOR OPERATING INSTRUCTION

Operate the auto-door in the power-on state.
Look for the press sign on the door. Press the button and hold to push the door out and
open it by hand. Before closing the door, make sure the top auto-scaling rod has retracted.
[image: ]
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 (
Do not close the door b
efore
 the auto-scaling rod retra
cts.
)




Note: In the power-off state, you cannot operate the auto-door. You can open the door from the crack directly with hand if needed.
Once the door is closed, you need to press the open key to open the door after an interval of 4 seconds, otherwise the door cannot be opened.


 (
OPERATION ANOMALIES
)

Ensure that there is power to the electrical supply plug by connecting another electrical appliance to it. Check fuse, if any. Make sure that the door is closed properly.

If your wine cabinet appears to be malfunctioning, unplug it and contact your after sales service. Any intervention on the cold circuit should be performed by a refrigeration
technician who should carry out an inspection of the circuit sealing system. Similarly, any intervention on the electrical circuit should be performed by a qualified electrician.
Notes: Any  intervention performed  by  a  non-  authorized  technician  will  lead  to  the warranty being considered as null and void.
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POWER FAILURES

In the event of a power interruption, all previous temperature settings are automatically retained and it will revert to a preset temperature setting.

Most power failures are corrected within a short period of time. An hour or two’s loss of power will not affect wine cabinet’s temperatures. To avoid sudden change of temperature while the power is off, you should avoid opening the door.  For longer period of power failure, do take steps to protect your wine.

Irrespective of the cause, if you notice either  abnormal temperature or humidity levels inside your wine cabinet, be reassured that only long and frequent exposure to these abnormal conditions can cause a detrimental effect on your wines.


 (
TROUBLESHOOTING GUIDE
)

Common problems may easily be solved, saving you the cost of a possible service call. Please read carefully the instruction manual and revert to troubleshooting guide chart.


	PROBLEM
	POSSIBLE CAUSE

	Wine cabinet does not
operate.
	Not plugged in.
The appliance is turned off.
The circuit breaker tripped or the fuse is broken.

	Wine cabinet is not cold
enough.
	Check the temperature control setting.
External environment may require a higher setting. The door is opened too often.
The door is not closed completely.
The door gasket does not seal properly.

	Turns on and   off frequently.
	The room temperature is hotter than normal.
A large amount of contents has been added to the Wine cabinet. The door is opened too often.
The door is not closed completely.
The temperature control is not set correctly.
The door gasket does not seal properly.

	The light does not work.
	Not plugged in.
The circuit breaker tripped or a blown fuse. The bulb is out of order.
The light button is “OFF” .

	Vibrations.
	Check to assure that the Wine cabinet is level.

	The Wine
cabinet seems to make too
much noise.
	The rattling noise may come from the flow of the refrigerant, which is normal.
As each cycle ends, you may hear gurgling sounds caused by the flow of refrigerant in your Wine cabinet.




27



	
	Contraction and expansion ofthe inside walls may cause popping and crackling noises.
The Wine cabinet is not level.

	The door will not close
properly.
	The Wine cabinet is not level.
The door was reversed and not properly installed.  The gasket is faulty. ( magnet or rubber is spoiled) The shelves are out of position.



	Standard features:
Compressor operated: R600a

	- Available in rated voltage/frequency:
220 - 240V, 50Hz

	- Automatic defrost

	- Humidity : 65% RH +/-10% RH

	- Black outer and inner finish

	- Internal light

	- Adjustable feet x 4

	- Triple layers glass door

	- Optional Common or Seamless stainless steel finish door frame or Full black glass door
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